{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":119,"n_cols":10,"rows_kept":119,"merged":[[0,0,0,9],[1,0,1,1],[2,0,27,0],[2,1,22,1],[2,2,8,2],[9,2,11,2],[12,2,15,2],[16,2,20,2],[21,2,22,2],[23,1,27,2],[28,0,28,9],[29,0,50,0],[29,1,35,1],[29,2,33,2],[34,2,35,2],[36,1,44,1],[36,2,39,2],[40,2,42,2],[43,2,44,2],[45,1,45,2],[46,1,50,2],[51,0,51,9],[52,0,78,1],[52,2,71,2],[72,2,78,2],[72,5,73,5],[76,5,77,5],[79,0,79,9],[80,0,108,0],[80,1,91,1],[80,2,82,2],[83,2,86,2],[87,2,89,2],[90,2,91,2],[92,1,94,2],[95,1,97,2],[98,1,108,2],[109,0,109,9],[110,0,112,0],[110,1,110,2],[111,1,112,2],[113,0,115,9],[117,5,117,9],[118,5,118,9]],"flags":["formulas_cached_only"]}
["2026年度舞台设备租赁服务报价一览表"]
["设备",null,"类型","序号","设备名称","参数要求","数量","单位","单价（元）","单位"]
["灯光部分","常用灯光设备","电脑灯",1,"摇头图案灯","满足舞台图案铺设的需求，具备定点功能",1,"盏",null,"元"]
[{"$nulls":3},2,"摇头染色灯","满足舞台染色的需求，色彩光斑均匀",1,"盏",null,"元"]
[{"$nulls":3},3,"电脑切割灯","适用于远距离面，舞台定点及特殊光源需求",1,"盏",null,"元"]
[{"$nulls":3},4,"三合一电脑灯","BSW三合一电脑灯，具备光束图案染色功能",1,"盏",null,"元"]
[{"$nulls":3},5,"摇头光束灯","需满足色彩饱和，亮度统一",1,"盏",null,"元"]
[{"$nulls":3},6,"玻璃材质logo片","满足对应图案灯或切割灯灯型",1,"个",null,"元"]
[{"$nulls":3},7,"铁片材质logo片","满足对应图案灯或切割灯灯型",1,"个",null,"元"]
[null,null,"LED灯珠",1,"LED PAR灯","R,G,B色，18颗3瓦灯珠，户外可防雨",1,"盏",null,"元"]
[{"$nulls":3},2,"洗墙灯","R,G,B色，满足户外防雨使用",1,"盏",null,"元"]
[{"$nulls":3},3,"城市之光","R,G,B色，满足户外防雨使用",1,"盏",null,"元"]
[null,null,"常规灯",1,"基础面光灯","COCO",1,"盏",null,"元"]
[{"$nulls":3},2,"ETC PAR灯","800W带遮飞",1,"盏",null,"元"]
[{"$nulls":3},3,"ETC灯（成像灯）","750W（根据活动需要，含0至5度镜头）",1,"盏",null,"元"]
[{"$nulls":3},4,"追光灯","1500W--3000W,色温可调，可加色纸",1,"盏",null,"元"]
[null,null,"特效灯",1,"单眼特效灯","R,G,B，三色，支持频闪功能",1,"盏",null,"元"]
[{"$nulls":3},2,"两眼特效灯","R,G,B，三色，支持频闪功能",1,"盏",null,"元"]
[{"$nulls":3},3,"四眼观众灯","常规色",1,"盏",null,"元"]
[{"$nulls":3},4,"激光灯","20W全彩激光灯",1,"盏",null,"元"]
[{"$nulls":3},5,"激光灯","25W全彩激光灯",1,"盏",null,"元"]
[null,null,"灯控台",1,"原装珍珠2010数字灯光控台","Avolites Pearl 2010 linghting Controller",1,"台",null,"元"]
[{"$nulls":3},2,"原装MA数字灯光控台","MA Lighting Controller",1,"台",null,"元"]
[null,"特效部分",null,1,"烟机","配烟油",1,"台",null,"元"]
[{"$nulls":3},2,"雾机","配泡泡油",1,"台",null,"元"]
[{"$nulls":3},3,"泡泡机","独歌",1,"台",null,"元"]
[{"$nulls":3},4,"干冰机","大干冰机，含干冰",1,"台",null,"元"]
[{"$nulls":3},5,"雪花机","可吊装",1,"台",null,"元"]
[]
["音响系统","音控台","数字调音台",1,"48路数字调音台","YAMAHA PM5D",1,"台",null,"元"]
[{"$nulls":3},3,"32路数字调音台","MIDAS M-32",1,"台",null,"元"]
[{"$nulls":3},4,"32路数字调音台","ALLEN&HEATH 32路",1,"台",null,"元"]
[{"$nulls":3},5,"32路数字调音台","Behringer X-32",1,"台",null,"元"]
[{"$nulls":3},6,"16路数字调音台","YAMAHA 16路",1,"台",null,"元"]
[null,null,"模拟调音台",1,"12路调音台","YAMAHA",1,"台",null,"元"]
[{"$nulls":3},2,"12路调音台","soundcraff ",1,"台",null,"元"]
[null,"话筒","无线手持话筒",1,"无线手持话筒","SHURE / Mipro /AMS/Sennheise",1,"套",null,"元"]
[{"$nulls":3},2,"无线手持话筒","SHURE / Mipro /AMS/Sennheise",1,"套",null,"元"]
[{"$nulls":3},3,"无线手持话筒","SHURE / Mipro /AMS/Sennheise",1,"套",null,"元"]
[{"$nulls":3},4,"无线手持话筒","SHURE / Mipro /AMS/Sennheise",1,"套",null,"元"]
[null,null,"会议话筒",1,"讲台有线鹅颈话筒","SHURE 或同级别话筒",1,"套",null,"元"]
[{"$nulls":3},2,"讲台无线鹅颈话筒","SHURE 或同级别话筒",1,"套",null,"元"]
[{"$nulls":3},3,"手拉手会议话筒（含主机）","SHURE 或同级别话筒",1,"只",null,"元"]
[null,null,"电容话筒",1,"枪声电容话筒","（含话筒专用支架）",1,"套",null,"元"]
[{"$nulls":3},2,"大振膜电容话筒","（含话筒专用支架）",1,"套",null,"元"]
[null,"点歌机",null,1,"点歌机",null,1,"台",null,"元"]
[null,"音响套装配置",null,1,"下乡慰问","小型线阵列：配置单十寸全频主扩、低音及反听音响",1,"套",null,"元"]
[{"$nulls":3},2,"广场演出","小型线阵列：配置单十寸全频主扩、低音及反听音响",1,"套",null,"元"]
[{"$nulls":3},3,"大型演出线阵音响（满足1000人）","中型线阵列：配置单十二寸主扩、低音及反听音响",1,"套",null,"元"]
[{"$nulls":3},4,"大型演出线阵音响（满足2000人）","中型线阵列：配置单十二寸主扩、低音及反听音响，根据场地情况需求适当增配",1,"套",null,"元"]
[{"$nulls":3},5,"超大型演出线阵音响（满足4000人以上2万人以下）","中型线阵列：配置双十二寸主扩、低音及反听音响",1,"套",null,"元"]
[]
["舞台部分",null,"舞台结构及物料部分",1,"铝合金边框舞台板及搭建","单块规格：1米以上正方形舞台板,可根据演出需要，任意扩展搭建；台高：60cm,80cm,100cm可调；舞台每平米载重大于500公斤；必须保证舞台搭建后，舞台的平整。舞台两侧各配备2米宽的阶梯。并对舞台在搭建与使用过程中的安全负责。",1,"㎡",null,"元"]
[{"$nulls":3},2,"舞台背景架（金属材质）","具备各种舞台宽、高尺寸的需要，任意组合；能适用舞台背景的镂空安装或者外蒙喷绘布等的安装；能在户外10级大风环境下安全使用；含该背景架在搭建、使用中的加固、保护所产生的一切费用。并对搭建与使用过程中的安全负责。",1,"㎡",null,"元"]
[{"$nulls":3},3,"灯光truss架","合金材质，满足净内宽17米以上跨度、同时能在跨度内任意点承载300㎏以上吊挂设备；能在户外10级大风环境下安全使用；（含升降设备）",1,"米",null,"元"]
[{"$nulls":3},4,"舞台地胶","3厘以上，接缝处平整，并对其安全负责。",1,"㎡",null,"元"]
[{"$nulls":3},5,"舞台地毯","必须与舞台面牢固粘合，对因其安全负责",1,"㎡",null,"元"]
[{"$nulls":3},6,"舞台地毯（阻燃）","满足消防阻燃安全要求、必须牢固粘合",1,"㎡",null,"元"]
[{"$nulls":3},7,"舞台地毯（加厚）","拉绒加厚款、必须牢固粘合",1,"㎡",null,"元"]
[{"$nulls":3},8,"灯光网架","配备必要的水平螺旋调节件",1,"根",null,"元"]
[{"$nulls":3},9,"帐篷（3m*3m）含围布","演员休息用（含固定设施）",1,"顶",null,"元"]
[{"$nulls":3},10,"帐篷（5m*5m）含围布","尖顶欧式帐篷",1,"顶",null,"元"]
[{"$nulls":3},11,"方凳","塑料方凳",1,"条",null,"元"]
[{"$nulls":3},12,"靠背椅","塑料靠背椅",1,"条",null,"元"]
[{"$nulls":3},13,"折叠椅","铁艺折叠皮套坐垫",1,"条",null,"元"]
[{"$nulls":3},14,"贵宾椅","含椅套",1,"条",null,"元"]
[{"$nulls":3},15,"IBM桌","1.83m长条桌",1,"张",null,"元"]
[{"$nulls":3},16,"单人沙发","白色皮沙发",1,"个",null,"元"]
[{"$nulls":3},17,"单人沙发","中南海沙发",1,"个",null,"元"]
[{"$nulls":3},18,"茶几","木制茶几",1,"个",null,"元"]
[{"$nulls":3},19,"铁马","1.2m*2m",1,"片",null,"元"]
[{"$nulls":3},20,"礼宾杆","一米栏",1,"个",null,"元"]
[null,null,"舞台制作部分",1,"舞台背景喷绘（3米机）","含按要求设计、制作、安装、拆卸、搬运",1,"㎡",null,"元"]
[{"$nulls":3},2,"舞台背景喷绘（5米机）",null,1,"㎡",null,"元"]
[{"$nulls":3},3,"KT板背胶材料","常用语讲台贴等",1,"㎡",null,"元"]
[{"$nulls":3},4,"舞台铁网镂空背景","含景片、文字制作、安装、拆卸、搬运",1,"㎡",null,"元"]
[{"$nulls":3},5,"木质舞美（板状）","含制作、搬运、安装、拆卸",1,"㎡",null,"元"]
[{"$nulls":3},6,"木质舞美（立体）",null,1,"m³",null,"元"]
[{"$nulls":3},7,"4阶合唱台",null,1,"m³",null,"元"]
[]
["屏幕部分","屏幕","室内屏",1,"P2室内高清全彩LED","Gloshine / Lightlink",1,"平方",null,"元"]
[{"$nulls":3},2,"P3室内高清全彩LED","Gloshine / Lightlink",1,"平方",null,"元"]
[{"$nulls":3},3,"P4室内高清全彩LED","Gloshine / Lightlink",1,"平方",null,"元"]
[null,null,"户外屏",4,"P3户外高亮防雨LED","Gloshine / Lightlink",1,"平方",null,"元"]
[{"$nulls":3},5,"P4户外高亮防雨LED","Gloshine / Lightlink",1,"平方",null,"元"]
[{"$nulls":3},6,"P6户外高亮防雨LED","Gloshine / Lightlink",1,"平方",null,"元"]
[{"$nulls":3},7,"P6户外高亮防雨透风LED","Gloshine / Lightlink",1,"平方",null,"元"]
[null,null,"导角屏",8,"P3导角屏","Gloshine / Lightlink，支持0-90°导角",1,"平方",null,"元"]
[{"$nulls":3},9,"P4导角屏","Gloshine / Lightlink，支持0-90°导角",1,"平方",null,"元"]
[{"$nulls":3},10,"P6导角屏","Gloshine / Lightlink，支持0-90°导角",1,"平方",null,"元"]
[null,null,"特殊屏",11,"地砖屏","Gloshine / Lightlink",1,"平方",null,"元"]
[{"$nulls":3},12,"冰屏","Gloshine / Lightlink",1,"平方",null,"元"]
[null,"投影机",null,1,"12000流明","EPSON / SONY",1,"台",null,"元"]
[{"$nulls":3},2,"10000流明","EPSON / SONY",1,"台",null,"元"]
[{"$nulls":3},3,"25000流明","EPSON / SONY",1,"台",null,"元"]
[null,"投影幕",null,1,"300寸","含支架",1,"块",null,"元"]
[{"$nulls":3},2,"200寸","含支架",1,"块",null,"元"]
[{"$nulls":3},3,"150寸","含支架",1,"块",null,"元"]
[null,"屏幕控制系统",null,1,"小型切换器","MIG 590",1,"台",null,"元"]
[{"$nulls":3},2,"基础控台","Jastron A6",1,"台",null,"元"]
[{"$nulls":3},3,"中型控台","MIG V8",1,"台",null,"元"]
[{"$nulls":3},4,"大型活动控台","Barco EC200",1,"台",null,"元"]
[{"$nulls":3},5,"融合拼接器","MIG H8",1,"台",null,"元"]
[{"$nulls":3},6,"融合拼接器","Watchout",1,"通道",null,"元"]
[{"$nulls":3},7,"融合拼接器","Barco E2",1,"台",null,"元"]
[{"$nulls":3},8,"播控系统","HIRENDER S3",1,"台",null,"元"]
[{"$nulls":3},9,"监视器/题词器","50寸液晶",1,"通道",null,"元"]
[{"$nulls":3},10,"高清信号传输","4K optical cable",1,"条",null,"元"]
[{"$nulls":3},11,"翻页器/远距离一拖二","Cuelight",1,"套",null,"元"]
[]
["策划设计服务","项目策划设计",null,1,"中大型活动策划设计服务","1、提供3D舞美设计方案，以及相应的施工图（尺寸图、材质图）；2、活动报备涉及的（座位图、安保点位图、人员疏散动线图）等；3、主视觉设计；4、延展设计：指示系统、节目单、图片视频直播画面等，主视觉相关物料的延展设计。",1,"场",null,"元"]
[null,"平面设计",null,2,"日常活动设计服务","主视觉版面设计，至少配合3次修改要求。",1,"场",null,"元"]
[{"$nulls":3},3,"日常活动设计（延展设计）服务","主视觉的延展设计，应根据采购人的实际需求在限额范围内弹性结算。",1,"场",null,"元"]
["注：以上设备配套的调光硅箱、直通电源箱、主电缆、配电箱及所有强弱电线缆、舞台乐队用电、安全防范措施，技术保障人员等根据演出配置，均不另行计费，报价已包含税率。"]
[]
[]
[]
[{"$nulls":5},"报价单位："]
[{"$nulls":5},"报价时间："]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}